#### Step 3: Create the PC-DMIS Program File and Import the DMIS File

- Create a new PC-DMIS part program.

- Import the measuring ChorusNT part program, specifying the MYRPOBE.PRB probe file created in the previous step.

- Usually Chorus measuring programs contain SNSLCT/ S(label) or SNSLCT/SA(label) statements. For self-calibrated wrists, you can explicitly specify roll and pitch angles in the SNSLCT label.

After PC-DMIS imports the DMIS file, the final PC-DMIS part program will have at the beginning the LOADPROBE/MYPROBE.PRB command, and for each SNSLCT statement the corresponding TIP command will appear with the correct A and B angles.