## Defining Probes

One of the first steps in part programming is to define which probes will be used during the inspection process. Because probe definition and calibration processes are often different depending on your specific configuration of PC-DMIS, this information is instead covered in the documentation set for your configuration. Consult the appropriate documentation set below for information on setting up, calibrating, and using an appropriate probe for your specific situation:

- PC-DMIS CMM

- PC-DMIS Vision

- PC-DMIS Laser

- PC-DMIS Portable

Defining probes uses the Probe Utilities dialog box.

Hint: Click this icon from the Wizards toolbar to access the PC-DMIS Probe Wizard.

More:

Understanding the Probe Utilities dialog box

Migrating Part Programs Between Machines Using PH10 and Tesa Star M Probes