#### Auto Wrist Toggle

This icon chooses the best wrist position to measure this Auto Feature's hits. Upon creation, it will automatically insert a tip command before the Auto Feature.

This icon tells PC-DMIS to choose the best wrist position to measure the Auto Feature. Upon feature creation, the software inserts the tip command before the Auto Feature.

- If the this icon is selected, PC-DMIS will choose a position that most closely approximates the best approach direction:

- - For edge and angle point features, the best approach direction is the average of the two surface vectors.

  - For corner point features, the best approach direction is the average of the three surface vectors.

  - For all other auto types, the best approach direction is the feature surface vector.

- If this icon is not selected, PC-DMIS will use the current wrist position for all hits made.

You can also turn this option on globally by selecting the Automatically Adjust Probe Head Wrist check box. See the "Automatically Adjust Probe Head Wrist" topic in the "Setting your Preferences" chapter.