### Basic Measurement Format for a Cone

The minimum number of hits for a cone is six. | Feature_name=FEAT/CONE,TOG1,TOG4,TOG5 THEO/TX,TY,TZ,TI,TJ,TK,TL,TD1,TD2 ACTL/X,Y,Z,I,J,K,L,D1,D2 MEAS/CONE,TOG3 ...
ENDMEAS/

TOG1= This field can be toggled between RECT / POLR.

TOG3= This value is user editable and is determined by the feature being measured. The HIT line is varied, based on the number of hits set up by the user. For example, 6 hits = 6 HIT/BASIC lines, 11 hits = 11 HIT/BASIC lines.

TOG4= This field can be toggled between IN / OUT.

TOG5= This field can be toggled between LENGTH / ANGLE.

...= As many hits as are necessary are entered at the ellipsis.

TD1,TD2= These are the cone's two theoretical diameters.

D1,D2= These are the actual measured values for the cone's two diameters