#### Adding Lines

In order to create an additional line within the location dimension:

1. Place the cursor in the desired location.

2. Press the ENTER key.

3. Type in the desired axis (X, Y, Z, D, R, A, V, T, L, S, H, M, PR, PA, PD).

4. Press the TAB or ENTER key.

PC-DMIS will then display the values for the added axis. PC-DMIS adds the new line depending on where the cursor is located. If the cursor is in the middle of a command, a new line is created below the current line. If the cursor is placed at the beginning of a command line, PC-DMIS will create the new line above the current cursor position.