## The Status Bar

The status bar displays the following:

1 - SD: This shows the standard deviation of the last feature measured.

2 - Line: This box displays a number that indicates the current line where the cursor is located in the Edit report. Col: This box displays a number that indicates the current column where the cursor is located in the Edit report.

3 - W: Angle of Rotary Table:

4 - Message Box: The left-most box displays instructions and other information regarding the current procedure or command.

5 - X, Y, and Z boxes: These boxes show the X, Y, and Z position of the probe. Clicking on any of the three coordinate displays within the status bar will cause the Auto Move Point dialog box to appear. (See "Inserting a Move Point Command" in the "Inserting Move Commands" chapter for additional information regarding DCC Move Point.)

6 - # of Hits: This shows the number of hits currently taken.

7 - IN/MM: This shows the current unit of measurement used for the part program.

8 - INS/OVR: - This box indicates the current editing function of the Edit report. It will display INS (for INSERT, meaning it inserts text at the cursor) or OVR (for OVERWRITE, meaning it overwrites any text encountered by the cursor).

Status Bar Manipulations

- To increase the size of the status bar, select View | Statusbar | Large. Due to its increased size, this large status bar will only display the Message and the XYZ boxes.

- To put the status bar back to its normal size, select View | Statusbar | Normal.

- To show or hide the Status bar, select View | Statusbar | None.