#### Leica Reset tab

Machine Options dialog box - Reset tab

Home button - Leica Tracker laser will Go Birdbath (for reflectors) or to 6DoF 0 position (for T-Probe).

Machine or Part coord. option - Select Machine if you are using Machine Coordinates, or Part coord. if you are using part coordinates.

Reset button - This is similar to the Aim button, but is used for machines without ADM. Click Reset to update the selected point with data from the new point position.

Aim button - Select a point from the Reset Point list and click the Aim to move the laser to the specified point.

Add button - Click the button to open the Point dialog box. Provide a Title and the XYZ values and click Create. The new point is added to the Reset Point list above. For example, you might have attached reflectors to positions on a car door. You could then name these positions Door1, Door2, Door3, etc.

Delete button - Select a point from the Reset Point list and click Delete. The selected point is deleted.

Use Default Reset - Select this option to use the Default Reset. If the beam is broken, the tracker will go back to the specified start position.

Set Default Reset - Select a point from the Reset Point list, and click Set Default Reset. This is now the Default Reset.

Aim Laser To Next Point - It will automatically move to the first point of the next feature in DCC.

Option Buttons - Not currently used

- Safety Position - Not currently used

- Go Birdbath - Not currently used

- Keep Last Position - Not currently used

- Go Point - Not currently used