#### Step 1 - Select the SP600 Probe Changer

To begin the calibration process, select Edit | Preferences | Probe Changer to open the Probe Changer dialog box.

Probe Changer dialog box - Type tab

To select the SP600 Probe Changer, follow these steps:

1. Once the Probe changer dialog box is open, select the Type tab.

2. Specify the number of different types of probe changers in the Number of probe changers box.

3. In the Active probe changer box, select the list item representing the probe changer to be defined. If this is the first probe changer, it will be listed as "Probe Changer 1: TYPE=None".

4. Select SP600 from the Probe changer type list.

5. Specify the Docking speed. The default value of 5% is appropriate for most machine configurations.

6. Click Apply to make this probe changer active and to load settings that are relevant to this probe changer. Other tabs become visible after you click Apply.

In the next step, you will define the location your probe body will move to when using the probe changer to switch probe components.

Next Step