#### Scanning after Adding Control Points

Once you've defined all the control points and created your scan, during execution, PC-DMIS does the following.

1. The scan will initially use the globally set Scan Speed and Point Density values.

2. As it scans along the path and passes within the parameters defined by the control points, the scan behavior changes as directed by the control points.

3. Once the scan is completed, the Scan Speed and Point Density will return to the globally set values.