### Step 9 - Review Calibration Results

Select the Slots tab on the Probe Changer dialog box, and you will see that calibration information now exists for the location of each of the calibrated ports.

Probe Changer dialog box - Slots tab with calibration results

When viewing the results, some things to watch for are the position of the rack and the spacing of the slots.

Results During Part Program Execution

- Probe entities that are added to each of the ports will be automatically picked up from that location whenever PC-DMIS executes a LOADPROBE command for that probe.

- The probe body will move to the mount point, then into the port, pushing the lid backwards. Then, using the magnetic attraction, it will load the new module and will continue measurement.

This calibration process only discusses the process for preparing ports for calibration. See the “Setting Up Probe Changer Options” topic in the "Setting Your Preferences" chapter for information about adding probe definitions to each of the ports.