#### IJK Edge boxes

These boxes are only available for the Edge Point and Line features. | The IJK Edge boxes define the approach direction (vector) for the edge hit or for the points of an auto line. This is a user supplied I, J, K measured vector. The I, J, K should always point away from the edge and be perpendicular to the edge that is being measured.

After you define a new value, PC-DMIS normalizes the vector, making its length one unit.

Icon | Description
| Swap Vectors
| Flip Vector
| Use Thickness