## Installation

If a wrist is installed on your CMM, PC-DMIS will add A and B axes to the X, Y, and Z readouts that are normally displayed. The wrist option must be turned on in the port lock for PC-DMIS to enable the wrist support. Because of the variety of infinite wrists and interfaces supported, you should consult with your software vendor for specifics on what PC-DMIS registry entries need to be changed (see the "Modifying Registry Entries" appendix for information on using the PC-DMIS Settings Editor to modify registry entries).

PC-DMIS will automatically query the controller and determine that the wrist is present.

More:

Notes for Renishaw PHS with Leitz Interface