#### Step 7 - Review Calibration Results

Once the DCC measuring finishes, select the Slots tab on the Probe Changer dialog box, and you will see that calibration information now exists for the location of each of the calibrated ports.

Probe Changer dialog box - Slots tab with calibration results

When viewing the results, some things to watch for are the position of the rack and the spacing of the slots.

This rack is not necessarily aligned parallel to any axis of the CMM. However, the X and Y values should show equal spacing between ports, roughly 53.5 mm apart. Also, the Z values should be nearly identical, since the slots are all at the same height. Significant deviations from these expectations might be due to a bad hit.

Results During Part Program Execution

- Probe entities that are added to each of the ports will be automatically picked up from that location whenever PC-DMIS executes a LOADPROBE command for that probe.

- The probe body will move to the mount point, then into the "unload" port (the port that used to contain the currently used probe entity), pushing the lid backwards. The current "puck", a black conical piece of hardware that connects to the bottom of the probe body, will be held in place by the rack while the probe body lifts away to detach.

- From there, the probe will move over to the next "load" position and the magnetic connection will automatically engage to load the new module.

- It will then move back to the rack’s mount point and from there will continue measurement.