### Laser Edge Point

Edge Point Auto Feature

To measure an edge point with a laser probe:

1. Access to Auto Features dialog box, and select Edge Point

2. Do one of the following:

1. Perform clicks on the cad to give the point a location and vector. Then manually enter any remaining information.

2. Move the machine to the point location using the Laser View tab on the Graphics Display Window. Next press the Read Point from Position button. Then manually enter the any remaining information.

3. Manually enter all of the theoretical x, y, z, I, j, k, etc.

3. As needed specify values for the Depth, Indent, and Spacer boxes. PC-DMIS will show a corresponding graphical visualization of the change in the Graphics Display window.

4. Enter the necessary information in the Probe Toolbox tabs. You will likely want to cycle through the Laser Scan, Laser Filtering, and Laser Clipping, properties tabs to enter the information.

5. Click the Test button if desired. Warning: The machine will now move!

6. Click the Create button and then Close.

More:

Edge Point Command Mode Text

Edge Point Specific Parameters