#### Boundary Points

PC-DMIS lets you define the boundary of a scan by typing the XYZ values for the individual boundary points directly, measuring the points using the laser probe, or using the CAD data.

Boundary Points and Vectors area

Boundary Points are not available or necessary for Free-form scans

You can change the column widths of the Boundary Point list by selecting the right or left edge of a column header with the left mouse button and dragging the edge to the desired size. This information is saved to your PC-DMIS Settings Editor each time they change.

More:

Setting Boundary Points by Typing

Setting Boundary Points Using the Measured Point Method

Setting Boundary Points Using the CAD Data Method

Editing Boundary Points

Clearing Boundary Points

Generate

Undo

Adding and Deleting Boundary Points