### Exposure and Gray Sum Settings by Feature and Material

Based on the feature type and the part material type the Exposure value found on the "Laser Probe Toolbox: Laser Scan Properties tab" and the Min and Max Gray Sum values found on the "Laser Probe Toolbox: Laser Pixel Locator Properties tab" should be adjusted according to the following table:

Exposure and Gray Sum Settings
Feature Based
Feature | Material | Exposure | Min Grey Sum | Max Grey Sum
Sphere | Tungstun Calibration Sphere | 120 | 10 | 300
Ceramic | 80 | 10 | 300
Gap/Flush | Sheet Metal | 150 | 30 | 300
White | 100 | 30 | 300
Blue | 120 | 30 | 300
Black | 450 | 10 | 300
Circle | Sheet Metal | 100 | 50 | 300
White | 100 | 50 | 300
Blue | 120 | 50 | 300
Black | 450 | 30 | 300
Aluminum | 80 | 50 | 300
Slot | Sheet Metal | 100 | 50 | 300
White | 100 | 50 | 300
Blue | 120 | 50 | 300
Black | 450 | 30 | 300
Aluminum | 80 | 50 | 300
Edge Point | Sheet Metal | 100 | 50 | 300
White | 100 | 50 | 300
Blue | 120 | 50 | 300
Black | 450 | 30 | 300
Aluminum | 80 | 50 | 300
Plane | Sheet Metal | 100 | 30 | 300
White | 100 | 30 | 300
Blue | 120 | 30 | 300
Black | 450 | 10 | 300
Aluminum | 80 | 30 | 300
Surface Point | Sheet Metal | 100 | 30 | 300
White | 100 | 30 | 300
Blue | 120 | 30 | 300
Black | 450 | 10 | 300
Aluminum | 80 | 30 | 300

Exposure and Gray Sum Settings