#### Scan Zoom Modes (for CMS Sensors)

CMS sensors provide you with an additional area called Zoom which is added to the bottom of the Laser Scan Properties tab of the Probe Toolbox. This area tells the sensor to work in predefined zoom modes, each mode being comprised of a specific combination of sensor frequency, data density, and Field of View (FOV) width.

Sample Zoom area

This area displays a table-like arrangement of option buttons arranged in columns and rows. Across the top, the "columns" show the data density. Along the side, the "rows" list the FOV width. You can only select proper combinations (those option buttons with a green background). Improper combinations are grayed out.

Hovering your mouse over any valid option button displays the selected scan mode information in a yellow ToolTip.

Sample ToolTip under the Mouse

Examples of CMS Scan Zoom Modes

Maximize your help viewer, and then click on the images below. Notice how different scan modes change the display in the Laser View tab:

4.1 Pts/mm and 124mm Width | 8.4 Pts/mm and 60mm Width | 16.8 Pts/mm and 24mm Width