### Laser Surface Point

Surface Point Auto Feature

To measure a square surface point with a laser probe:

1. Access the Auto Features dialog box, and select Surface Point.

2. Do one of the following:

1. Perform clicks on the cad to give the point a location and vector. Then manually enter any remaining information.

2. Move the machine to the point location using the Laser View tab of the Graphics Display Window. Next press the Read Point from Position button. Then manually enter the any remaining information like the snap value, etc.

3. Manually enter all of the theoretical x, y, z, i, j, k, snap value, etc.

3. Enter the necessary information in the Probe Toolbox tabs. You will likely want to cycle through the Laser Scan, Laser Filtering, and Laser Clipping, properties tabs to enter the information.

4. Click the Test button if desired. Warning: The machine will now move!

5. Click the Create button and then Close.

More:

Surface Point Specific Parameters

Surface Point Command Mode Text

Auto Surface Point Path