#### Parameter Change

Measurement Speed

- Move Speed – Supported.

- Touch Speed – Unsupported for systems that use a fixed feed rate for measurement moves. Supported for macro sets that allow setting feed rates for measurement moves, for example the Blum macro set.

- Scan Speed – Unsupported.

- Acceleration – Unsupported. This is a machine service parameter not accessed by operators or programmers.

Probe

- Manual / DCC Mode – DCC only is supported. Manual operations are not translated.

- Probing Parameters – All are Unsupported. Probing parameters are defined within the Probing macros. Probing speed, prehit and retract distances are supported in PC-DMIS NCI.

- Auto-Relative Measure – Unsupported. Supported in PC-DMIS NCI

- Prehit and retract distances – Supported.

Clamp Value

- Unsupported.

Temperature Compensation

- Manual compensation is unsupported. There is no mechanism in PC-DMIS NC for the operator to enter parameters in a running CNC program for manual compensation.

- Automatic compensation is unsupported via PC-DMIS NC.

NC-100 Video Settings

- Unsupported.