### Step 4: Verify the Rotary Table Calibration

To verify your Rotary Table calibration:

1. Select the Operation | CNC Programming | Create CNC Program menu option to post out the calibration program.

2. Open the CNC Server program.

3. Click Download Program and browse and select the newly created CNC program.

4. Click Analyze and execute the Calibration program on the NC machine.

5. Note the updated calibration information in the Rotary Table Setup dialog box in PC-DMIS after the calibration is complete. You may wish to add dimensions for the calibration program so as to view the results of the calibration in a report.

6. Check the Calibration - Create a sphere measurement program with the rotary table enabled. In this program, the sphere will always be at zero degrees in PC-DMIS, but the location of each measurement will deviate by the error in calibration of the table.