#### Automatic Features

Common Items

- Permanent Hits and Spacer – Partially Supported. Runtime sample hits will be taken but will not be used to modify the path. They will only be used in the Analysis phase.

- Initial Hits – Unsupported. These are learn-time sample hits. There is no learning function in V1.0.

- Re-Measure – Supported. However, there may be no benefit to re-measuring using the same path.

- Read Position – Unsupported. Supported in PC-DMIS NCI.

- Auto PH9 – Unsupported. 5 axis machine tools with multi-axis wrists may be supported in later versions. Supported in PC-DMIS NCI.

- On Error – Unsupported. PC-DMIS will be operating in a Server mode where the Operator will generally not see the screen. Supported in PC-DMIS NCI.

- Relative Measurement – Unsupported. This requires path modification based on measurement. Supported in PC-DMIS NCI.

- NOMINALS – FINDNOMS – MASTER – VECTOR list. NOMINALS only supported. Supported in PC-DMIS NCI.

Circle

- Circular Move – Supported. The path will be generated with straight line segments by PC-DMIS when only protected moves are allowed. Circular moves are supported in the major machine axis planes XY YZ ZX if the NC controller can perform them. Unsupported in PC-DMIS NCI which only works with straight line moves.

- Find Hole – Unsupported. Requires controller based path generation. Supported in PC-DMIS NCI.

Cylinder

- Find Hole – Unsupported. Supported in PC-DMIS NCI.

- Circular Move – Supported for unprotected motion. Supported in PC-DMIS NCI.

- Use Theoretical – Supported.

Cone

- Circular Move – Supported. Unsupported in PC-DMIS NCI.

Line

- For CMT Features Only – Unsupported.

Corner Point

- Supported since the path is not dependent on measurements.

Angle Point

- Supported since the path is not dependent on measurements.

Edge Point

- Unsupported. The points on the edge are determined by the surface point(s) which is a dynamically generated path. Supported in PC-DMIS NCI.

High Point

- Unsupported. Supported in PC-DMIS NCI.