### Step 7: Execute the NC Program File

1. Start execution of the NC program.

2. During execution, the NC program file will load the probe and proceed to measure the features defined in your part program.

3. Measured points are sent to the server computer from the NC controller.

4. PC-DMIS CNC Server parses the received lines from the controller. Each line contains a command identifier, a machine identifier, and possibly some other information.

Next Step...