### Step 1: Define the Laser Probe

1. Open an existing part program, or create a new one.

2. Select the Insert | Hardware Definition | Probe menu option to open the Probe Utilities dialog box (this dialog box will automatically appear whenever you create a new part program.)

Probe Utilities dialog box

3. Define a probe configuration that uses the CONTOUR probe and the appropriate Romer arm inside the Probe Utilities dialog box. The type of Perceptron Contour probe is specified in the SetUp Options dialog box.

Next Step ...