### Step 3: Check the Calibration Results

Click on the Results button in the Probe Utilities dialog box. The Calibration Results dialog box appears.

Calibration Results

PC-DMIS records several things from the calibration in this dialog box. Take a look at the maximum, average, and standard deviation values. The Average Error should be around 0.05mm. The Maximum Error should be around 0.15mm.

If the results look correct, click the OK button to close down the Calibration Results dialog box.

You are now done setting up and calibrating your laser probe. You should now have access to all laser-related functionality.

Note: If the calibration exceeds the tolerance value defined in the standard_deviation_limit registry entry, PC-DMIS adds a line of text that says, "Standard deviations for the probe calibration exceed limit" in the Calibration Results dialog box