## Total Station Interface

The parameters that control how PC-DMIS interfaces with the Total Station interface can be configured by selecting the Edit | Preferences | Machine Interface Setup menu item. This opens the Machine Options dialog box. The following tabs are available:

- Instrument Information Tab

- Comm Tab

- Reset Options Tab

- Instrument Options Tab

- Environmental Parameters Tab

- Debug Tab

Instrument Information Tab

(Documentation Pending)

Comm Tab

(Documentation Pending)

Reset Options Tab

On Break

This area lets you determine what happens when the laser beam from the Total Station to the probe is broken.

- Turn on laser pointer - This option turns on the laser pointer. See Laser Pointer ON/OFF menu item discussed in the "Total Station Menu" topic for more information on the laser pointer.

(Documentation Pending)

Instrument Options Tab

(Documentation Pending)

Environmental Parameters Tab

(Documentation Pending)

Debug Tab

See the "Generating a Debug File" topic in the Core PC-DMIS documentation.