### Other PC-DMIS Menu Items

Operation Menu

End Feature (END): Tells PC-DMIS that the amount of hits for the feature has been reached and the feature can be calculated.

Erase Hit (ALT+-): Deletes the last measured hit.

Take Hit (CTRL+H): Measures a stationary T-Probe or Reflector position, based on the measuring time specified in the "Sensor Configuration tab" of the Machine Options dialog box.

Move To: Accesses the Move Point dialog box, allowing you to insert a MOVE/POINT command into the part program. See the "Inserting a Move Point Command" in the core documentation for more information.

Start/Stop Continuous Mode (CTRL+I): Starts/Stops a scan, based on the basic scan settings found on the Probing tab of the Parameter Settings dialog box (Edit | Preferences | Parameters). The default value for Distance delta provides a continuous distance separation of 2mm.

Note: The AT401 does not support the Start/Stop Continuous Mode but it can be used on other Leica devices.