## GOM Interface

The GOM interface is used with the CTR, GOM, and Krypton machines. This interface works via a serial port. A generic parser can be used to adapt the interface to work with other manual machines where the format of data being received is known. Traconsa, Layout, and Manual Mitutoyo machines can be used in this manner with additional registry values (see the MIIM).

Before starting PC-DMIS, rename the GOM.dll to interfac.dll.

The Machine Option dialog box has three tabs for the GOM interface:

Controller tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 9600 Baud, No parity, 8 data bits, and 1 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).