### Sensor Configuration tab

Machine Options dialog box - Sensor Configuration tab

Absolute Distance Meter (ADM)

- Target Stability Tolerance: This tolerance (between 0.005 and 0.1 mm) determines the maximum range of movement of a reflector target during ADM measurements. Values beyond this range will show an error message.

- Time Frame For Retry: Sets the period of time for determining target stability. If the target is stable, an ADM measurement is taken.

- Number of Retries: Sets the number of attempts for an ADM measurement before aborting, because the stability of the target has exceeded the given tolerance.

Search Settings: If any of these search criteria are not met then the search process is aborted.

- Spiral Search Diameter: Diameter in which to search for the target.

- Abort Criteria: Time in which the target should be found.

- Distance to Point: Distance at which to search for the target.

Go Birdbath: The Leica Tracker will rotate to the Birdbath position in the Clockwise or Counter Clockwise direction from its current position.