### Feature End Read Time

Determines the amount of delay before reading the current position. This value is used for hard probes measuring features during execution. This delay helps to determine the direction vector for machines that do not have a done button to determine the direction vector.

Entry Name: FeatureEndReadTime

Entry Type: Whole Number specifying time in milliseconds. Default value is 500 (1/2 second).