### DCC End Ang

Allows you to define the default value for the End Ang option that will be used when an Auto Feature is created. This is a user supplied angle in decimal degrees. This value is used for Contact probes while the "EndAngle" value is used for Vision probes.

Entry Name: DccEndAng

Entry Type: Real Number to specify the angle in degrees. Default value is 360.

Note: It is important to remember when entering starting and ending angles that the IJK vector always looks down the centerline, and that PC-DMIS measures DCC circular features in a counterclockwise direction.