### Auto Wrist

Allows you to enable the automatic selection of the best probe tip angle to use for measuring the related feature. This angle will most closely relate to the approach vector for the feature. This corresponds to the PH9 option in the Auto Feature dialog box. If this option is set to FALSE (0), PC-DMIS will use the current tip angle.

Entry Name: AutoWrist

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.