### Sensor Clip Left Percent

Provides the left edge of the clipping plane as a percentage of your laser sensor's field of view. The clipping plane allows you limit the amount of data that is collected form your laser sensor. For example, a value of 15 would eliminate the first fifteen percent from the left edge of the sensor's entire field of view, while a value of 0 will use all data up to the left edge of the sensor's field of view.

Entry Name: SensorClipLeftPercent

Entry Type: Real Number to specify percentage. Default value is 0.