### Slave Mount (XYZ)

This value is not used.

These three values define the XYZ location that is used for a Mount Point for the slave arm. Mount points are safe locations where the arms will move each time that the system is used. To determine what these values should be, move the ram to the position that you want to use as the mount point for your slave arm and enter the XYZ values to their respective registry values.

Entry Name: SlaveMount(XYZ)

Entry Type: Real Number to specify (XYZ) mount point location. Default value is 0.

Common situations when you would use mount points include:

- After calibration

- Pulling a fixture out

- Recovering a column

- Calibrating the system

Note: On the slave computer, you need to enter the same values into the MountX, MountY, MountZ, that you put into the SlaveMountX, SlaveMountY, and SlaveMountZ, entries in the master computer's registry