### Renishaw Circle Scan Uses Hssdat

When this option is set to TRUE (1), PC-DMIS sends a distinct set of points defining the feature measurement path to the controller. Otherwise, when this value is set to FALSE (0), PC-DMIS will send the feature specific parameters to the controller.

Entry Name: RenishawCircleScanUsesHssdat

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.