### V_Rotab Table Num Spheres

If desired, the sphere may be measured in more than three angular positions when calibrating an infinite rotary table. This setting defaults to zero, in which case it’s not actually used and the angular positions for the calibration come directly from the calibration dialog. If this setting is greater than zero a full 360 degree rotation is divided into this many equally spaced measurement positions. If used this should be set to at least three.

This option is used for Table V.

Entry Name: RotabTableNumSpheres

Entry Type: Character String specifying number of spheres. Default value is None ( ).