### Scan Dialog Single Pnt

PC-DMIS will make each hit a measured point and insert it into the part program. This sequence will happen after the manual scan has been reduced. If the scan is in DCC mode, it will take place after the scan has been learned. This option is enabled when set to TRUE (1).

Entry Name: ScanDialogSinglePnt

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.