### Transfer Point

This value is not used.

Determines the a "Y" location that is accessible from both arms. To determine this location, move the ram to the Y position where you want the transfer of the columns from one arm to the other to occur. The "Y" value should be entered as the TransferPoint setting. PC-DMIS should give you a valid position for this setting that will work for both sides of the machine. If you do alter this setting, make sure that it can be reached by both arms otherwise you will be unable to transfer columns from one arm to the other.

Entry Name: TransferPoint

Entry Type: Real Number to specify the Y location for column transfer. Default value is 0.