### Stable Probing Distance

This provides the distance after which a stable probing hit will be triggered if Stable Probing mode is used within the PC-DMIS Portable software. This will only trigger a hit if the elapsed time also exceeds the value specified in the StableProbingTimeDelay entry.

Entry Name: StableProbingDistance

Entry Type: Real Number to specify distance in millimeters. The default value for SMX and Leica are both 1. The default for LeicaTPS is 2.