### Normal-(XYZ)

These values indicate the default direction of the normal vector that is displayed in the Pointcloud Operator dialog box. The direction value is defined with the NORMAL parameter in the Edit Window.

Entry Name: Normal-(XYZ)

Entry Type: Real Number specifying IJK values. Default values are X(I)=0, Y(J)=0, & Z(K)=1.

See the "CROSS SECTION" topic of the PC-DMIS Laser help file for more information.