### DEA Dual Drive Mode

This value should only be set to TRUE for large DEA gantry machines (such as Delta and Lambda) that may have the main axis (X in DEA convention, Y in Brown & Sharpe convention ) driven by two motors, one on each side of the carriage. In this case, the controller has also an additional axis to power that motor and gather counting signal from the related additional reader.

Entry Name: DEADualDriveMode

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is 0.