### Screen Capture Type

Determines the Type or images that will be captured for the SCREENCAPTURE.RTP for Laser or Vision Auto Features. The "ScreenCaptureQuality", "ScreenCaptureScale" and "ScreenCaptureTime" values are also used to determine the properties of the captured image.

Entry Name: ScreenCaptureType

Entry Type: Whole Number to specify which images will be captured. Default value is 0.

Value Key:

0 | NO | No screen captures will be included
1 | CAD | Include the image from the CAD View in the report.
2 | LIVE | Include the image from the LIVE View in the report. This is the most useful view to capture and include in your report for Vision machines. This is not available for Laser Auto Features.
3 | BOTH | Include images from both the Live View tab and the CAD View tab in the report. This is not available for Laser Auto Features.