### DCC XYZ2_1

Provides the default "Y" or "A" (angle) value for the for the end point of a line auto feature. The value will represent Y value when the "Cartesian" value is set to TRUE (1), and R when it is set to FALSE (0). This value and the "DccXYZ2_0" and "DccXYZ2_2" values are used for Contact probes while the "Point2(XYZ)" values are used for Vision probes.

Entry Name: DccXYZ2_1

Entry Type: Real Number to specify the Y or A value. Default value is 0.