### (XYZ) Auto Shutter Stage Drift Allowance

Provides the allowance for acceptable stage drift. During point detection, the stage position is recorded at the time the point detection command is issued. If at the time of the point detection command completes the stage position in the (XYZ) axes differs from the recorded stage position and this difference is greater than these XYZ values, PC-DMIS considers the stage to have drifted.

This value is only evaluated when "AutoShutterEnable" is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

Entry Name: (XYZ)AutoShutterStageDriftAllowance

Entry Type: Real Number to specify allowable distance. Default value is 0.00001 for X & Y and 0.00002 for Z.