### Auto Shutter Enable

When this option is set to TRUE (1), PC-DMIS Vision will detect when a target is ready to measure based upon the criteria defined in the following values:

- AutoShutterStageDriftRetries

- AutoShutterStageSettleTime

- AutoShutterTimeToFire

- AutoShutterTimeToFireNth

- AutoShutterTimeToFireOnFovEntry

- AutoShutterTimeToFireStageDrift

- (XYZ)AutoShutterStageDriftAllowance

When the defined criteria is met, the feature will automatically be measured. See the "Setting up the Live View" topic in the PC-DMIS Vision documentation.

Entry Name: AutoShutterEnable

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.