### DCC In Out

Use the DccSphereInOut value to affect this change rather then this value. This value is not used.

This value allows you to define the default value for the In/Out option that will be used when an Auto Feature is created. The In and Out value tells PC-DMIS whether to construct the sphere as an internal or an external sphere.

Entry Name: DccInOut

Entry Type: Whole Number to specify Internal Sphere (0) or External Sphere (1). Default value is 0.