### Send Calibration Results Files

When set to True, the calibration results files are transmitted between arms of a multi-arm system.

Entry Name: [SendCalibrationResultsFiles]

Entry Type: Possible values are True (default value) or False. When set to True, the calibration results files are transmitted between arms. When set to False, the calibration results files stay on the arm where the probe calibration has been performed.

Example: Calibrating a probe on the slave arm in standalone mode. When entering in Master/Slave mode the calibration result file is copied to the master arm.