### PTP_Sample Hits

Use the DccPermHits value to affect the permanent hits value respectively. ???? There are now values for each feature type. How are these used versus the DccPermHits value that is shown as a reference.

The Initial and Perm lists allow you to select the number of sample hits taken for the auto feature. These hits are used to measure the plane around the nominal point location.

· The Initial sample hits are taken only on the initial measurement of the feature during execution of the part program.

· The Perm sample hits are used for all subsequent measurements during execution of the part program.

The following table lists the auto features that use sample hits and how the sample hits are used in that feature's measurement.

Entry Name: SampleHits

Entry Type: Whole Number to specify … Default value is 0.