### Cross Section Profile Dimension Distribute Points Uniformly

This entry determines whether or not profile dimensions interpolate curves as uniformly spaced points onto cross section COPOPER points.

Entry Name: CrossSectionProfileDimensionDistributePointsUniformly

Entry Type: Whole number of 0 or 1.

- If this entry is set to 1, when you generate a profile onto a cross section COPOPER, PC-DMIS interpolates a curve on the cross section points and the points in the COPOPER are replaced by uniformly distributed points on the curve.

- If this entry is set to 0, then no curve interpolation takes place and any profile dimensions use the original COPOPER points.