### DCC Depth

Allows you to define the default value for the Depth option that will be used when an Auto Feature is created. A depth value is used for measuring sample hits. The sample hit is taken at a distance from the feature you are measuring. The behavior of this function differs depending on the Auto Feature type. See the section on "Depth Box" topic in the core PC-DMIS documentation for more information. This value is used for Contact probes while the "Depth" value is used for Laser probes.

Entry Name: DccDepth

Entry Type: Real Number to specify distance. Default value is 0.