### Wrist B Angle Start

Provides the starting B angle used for the calibration of your wrist device. As part of the calibration process, you need to calibrate wrist positions in a pattern of at least three A angle positions by at least three B angle positions for a total of nine sphere measurements.

Entry Name: WristBAngleStart

Entry Type: Real Number to specify the starting B angle. Default value is -180.